**DO NOT MOVE THE AXES WITH PRINTER POWERED OFF**

You **will** burn all the stepper drivers and will be on the hook for replacing them. They’re expensive.